Upgrading from 5.x firmware to 6.x firmware requires a calibration cycle.  Please contact support@quarch.com for help with this.

If you are already on the later PPM Plus firmware (version 6.000 and higher) then use the QTL1999 6.x folder

Check the firmware version using the *IDN? command